**DS4 Drop Part II**

**LAB 5**

**SECTION 2**

**Gavin Monroe**

**SUBMISSION DATE:**

**10/14/17**

# Problem

**Problem 1:** How much difference tends to occur in drops in the lab area? From the 2nd floor?

There isn’t a huge difference but I would say there is definitely a difference regarding maybe the accuracy of measurement. The Lab area is more controlled since we are literally the ones who are dropping it, but with the second floor its already set, all the data is there. I would say with the lab area, the distance was a constant small distance, while for the 2nd floor it was a distance set with the csv file.

**Problem 2:** How far is it from the second floor railing to the bottom floor according to your code?

New Equation:

Compensating for air resistance, the fall was **39.514 meters**.

Old Equation: 0.5 \* (v \* pow(sec, 2))

Compensating for air resistance, the fall was **79.659 meters.**

With this new equation you can see how much more accurate it is.

**Problem 3:** What issues arose in implementing Part 2?

I used the “real” equation to find distance for a falling object last lab, so this ;ab I had to go back to the previous lab and used the old equation(0.5 \* (v \* pow(sec, 2))) to find the difference for each fall difference. I made sure to do some research on finding the difference for two numbers just too make sure I got the right difference. There was two equations I had to use for this new part two lab, and 4 equations altogether. I also ran into numbers not lining up so I went back and rewrite some equations so the compiler could understand it better.

# Analysis

I needed to overall look at the old placement to output the new one, I needed to find the overall difference along with calculating the distance with a new equation.

# Design

Used 4 simple equations in a total of 4 different functions to help input and display information accordingly.

# Testing

In testing I had to find the small mistakes I made and go back and fix them. These mistakes were important to fix due to the accuracy of my numbers. Needed to use the correct numbers with the correct equations.

# Comments

I loved this challenge just because of the new angle we took on it.

# Source Code

/\* SE 185 Lab 5 Wrapper Program

Gavin Monroe

Fletcher Smith

\*/

#include <stdio.h>

#include <math.h>

#define TRUE 1

/\* Put your lab 4 functions prototypes here, as well as the prototype for lab 5 \*/

double mag(double x2, double y2, double z2);

void findFall(double ayInput);

void outputInfo(int oldd, int neww, double tm, double aTime);

void calcTime(int tm, int on);

void calcDistance(int tm, int on);

//Detect Change Vars

int d;

int d2;

//Distance & Time

double dist;

double dist2;

int start = 0;

int beforeTime;

double afterTime;

int main(void) {

int t;

double ax, ay, az;

while (TRUE) {

fflush(stdout);//Flush Code

scanf("%d, %lf, %lf, %lf", &t, &ax, &ay, &az );//Grab Input

d2=d;//set old orientation.

findFall(mag(ax, ay, az));//Find Direction which the controller is facing.

outputInfo(d2, d, t, afterTime);//Output Result.

calcTime(t, d);//Output dots

calcDistance(t, d);//Get Distance

}

return 0;

}

double mag(double x2, double y2, double z2){

/\* CODE SECTION 1 \*/

double sqrtX = pow(x2, 2);

double sqrtY = pow(y2, 2);

double sqrtZ = pow(z2, 2);

return sqrt(sqrtX + sqrtY + sqrtZ);

}

void calcTime(int tm, int on){

int varTime = tm % 100;

if (varTime == 0 && on == 1){

printf(".");

}

if (varTime == 0 && on == 2){

printf("!");

}

}

void calcDistance(int tm, int on){

if (on == 2){

double sec = tm - beforeTime;

sec = sec / 1000;

afterTime = sec;

double v = 9.8;

dist = v \* sec;

dist2 = 0.5 \* (v \* pow(sec, 2));

}

}

void findFall(double ayInput){

if (ayInput != 0 && start == 0){

start = 1;

d = 1;

}

if (ayInput >= 0.5 && start == 1 && d==1){

d = 2;

}

if (ayInput < 0.5 && start == 1 && d == 2){

d = 3;

}

}

void outputInfo(int oldd, int neww, double tm, double aTime){

if (oldd!=neww){

if (neww==1){

printf("Ok, I'm now receiving data.\nI'm Waiting");

}

if(neww==2){

beforeTime = tm;

printf("");

}

if(neww==3){

double dist3 = (dist + dist2) / 2;

int perc = ((dist2 - dist) / dist3) \* 100;

printf("\nCompensating for air resistance, the fall was %3.3lf meters.\nThis is %d%% less than computed before.", dist, perc);

}

if(neww==4){

printf("RIGHT\n");

}

}

}

# Screen Shots

